Function optimization description

①Sensor Optimization: 
Fixed reading drift. Actual temperature = Reading - 4°C for enhanced data accuracy.​

②Auto Defogging Iteration (PWM1 Interface):
Intelligently adjusts thresholds based on ambient temperature, featuring lag-free temperature control and more efficient defogging:​
Ambient temp > 15°C: Threshold = Dew Point + 7.5°C​

0°C ≤ Ambient temp ≤ 15°C: Threshold = Dew Point + 10°C​

Ambient temp ly set threshold to 5°C​

③Heating Control Optimization:
Default 97% power output on startup. Users can customize PWM gear when the heating belt hasn’t reached the protection point.​

New Feature​

Power-off Save for Settings: 
The system automatically saves settings every 5 seconds to prevent data loss in regular use. (Note: Data may not be saved if power is cut off immediately after settings are changed.)